**Seizmik Full Vented Windshield for the Polaris RZR XP Pro**

**Fitment: Polaris RZR XP Pro (2 and 4 seat models)**

**Part #: 26103**

**Material:** Double Sided Hard Coated Polycarbonate

**Features**

* **2-Side Hard Coated Polycarbonate Windshield**—Made to withstand more impact and resist scratching.
* **Innovative Windshield Vents:**
	+ Made of super-durable glass-filled nylon
	+ Gasket sealed against water intrusion
	+ Fully adjustable easy-to-use louver for variable airflow
	+ Two vents per windshield
* **Glass-filled Nylon Clamps—**Super strong and low profile, but do not interfere with other accessories.
* **Automotive Grade High Deflection Bulb Gasket—**Surrounds the lower edge of the windshield to protect against scratching the RZR XP Pro hood panels
* **Versatile—**Works with most roofs.
* **Seizmik Compatible:** Works with SEIZMIK® accessories: mirrors, light bars, etc.
* **Trailerable—**Up to 65mph when properly prepared.

Seizmik’s Versa-Vent windshield for the RZR XP Procomes equipped with two cleverly designed vents that let the driver and the passenger independently control the amount and direction of airflow. The vents have been mounted at the top of the windshield for better viewing out of the RZR XP Pro.

The vent is made of glass filled nylon, so it’s incredibly durable. The scoop on the front gathers up air off the windshield and re-directs it to inside the vehicle so even at very slow speeds there is a surprising amount of air that can come through the vent. The design of the scoop and the gasket between it and the windshield keeps precipitation out while still allowing airflow in—as much or as little as either the driver or passenger desires.

**Video URLs:**

Seizmik Versa Vent - Airflow: https://youtu.be/PChSDdQ6NdU