WINDSHIELD - VERSA-FOLD - UV RESISTANT POLYCARBONATE

SEIZMIK PART #: 23078 (Replaces 23076)

FITMENT INFO: Polaris Full Size Round Tube Ranger (2009-18)

The Seizmik UV Resistant Polycarbonate Versa-Fold Windshield for the 2009-18 Polaris Full Size Round Tube Ranger features a full perimeter gasket and quick release/secure composite levers allowing the windshield to be quickly folded down or up without the need for tools or leaving the vehicle's cab. 

Additions features include:

•	0.220" thick UV resistant polycarbonate
•	No drilling required for installation
•	Mounting hardware included
•	Full perimeter seal design (no gap between windshield and roof)—seals as good as any full windshield
•	Automotive grade high deflection bulb gasket around entire windshield perimeter insures best in class seal
•	Top folds against the bottom, nothing contacts the hood
•	Quickly release/secure upper windshield section with simple twist of 2 composite levers – no tools required
•	Top windshield held in folded position securely and easily with 2 heavy duty captive rubber plugs
•	Mechanically attached UV protected transparent hinge is durable and replaceable
•	Trailerable to 65mph when ‘folded down’ and properly secured