Seizmik Hard Coated Polycarbonate Rear Windshield for Polaris RZR Pro XP

Fitment: Polaris RZR Pro XP (2 Seat Models only)

Part #: 26105					

Material: Hard Coated Polycarbonate

Features
•	Hard Coated Polycarbonate Windshield—.210” thickness for rigidity and impact resistance
•	Prevents Backdraft—helps prevent dust and debris created by the changes in airflow from front windshields from entering the cab	
•	Contoured Fit—specifically designed to work with the angles of the rear opening on the RZR Pro XP
•	OEM Compatible—works with the following OEM parts: Aluminum Roofs (Part # 2883743-color designator or Part # 2883961-458); Pivoting Spare Tire Carrier (Part # 2884907-458); Forward Cargo Box (Part # 2883751); and Stage 4 Audio Upgrade Speakers (Part # 2884255)
•	Two Piece Design—creates a flat rear surface for distortion free viewing and clarity
•	Automotive Grade High Deflection Bulb Gasket—surrounds the edges of the windshield to protect against element intrusion
•	Glass Filled Nylon and Zinc Plated Hardware—for corrosion resistance and durability
•	Cast Aluminum Hardware Accents—for aesthetics and a finished look
•	No Drilling or Cutting Required
•	Trailerable—when properly prepared

Ride in comfort, no matter the weather, with Seizmik’s Rear Windshield for the Polaris RZR Pro XP (2 seat models only). Constructed from .210” hard coated polycarbonate. Designed and contoured to fit the profile of the RZR Pro XP and works with the following OEM accessories: Part # 2883743-color designator or Part # 2883961-458); Pivoting Spare Tire Carrier (Part # 2884907-458); Forward Cargo Box (Part # 2883751); and Stage 4 Audio Upgrade Speakers (Part # 2884255). 

*Does not work with Polaris Polycarbonate Roof (Part # 2883928)