UTV WINDSHIELD & HEADLIGHT WIPER WASHER KIT

SEIZMIK PART #: 30011

FITMENT INFO: For ANY Hard Coated Polycarbonate Windshield (Hard Coated Poly Only!!)

WARNING: Installation requires drilling holes your windshield.  Please read directions carefully and install AT YOUR OWN RISK.  Only attempt to install on hard coated polycarbonate windshields. Acrylic windshields will most likely crack if you attempt to install this kit. DO NOT attempt to install in glass.

The UTV Windshield & Headlight Wiper Washer Kit from Seizmik includes: wiper motor assembly; wiper arm & blade; pump; washer fluid reservoir; hose & fittings; wire harness; and mounting hardware. Equipped with dual, independently adjustable jets, 110º of wiper range motion to cover the entire driver's side of the windshield, and a 2 speed motor with an automatic park feature to position the blade up and out of the way when turned off. Features include:

•	14” AUTOMOTIVE WIPER BLADE—May be replaced with a standard style wiper blade
•	WIPER MOTOR ASSEMBLY—2 speed motor with automatic park position
•	STURDY STEEL BACKING PLATE—Heavy Duty mounting structure with rubber vibration isolation bumpers against windshield
•	HOSE—16’ long hose provides enough length to place jets in a number of locations
•	1.5 QUART RESERVOIR—Enough capacity to get the job done
•	4 SPRAY NOZZLES—Independently adjustable, dual jets in each nozzle
•	PLASTIC HOSE FITTINGS—Multiple choices for various configurations
•	SIMPLE INSTALLATION—Position wiper on your windshield, then locate the 2 points to drill